Problem Report PR-004

HW part: HW0002

HW rev: R002

Description: PCB hardware is not able to independently control MIDI THRU.

Analysis to demonstrate the problem:

1. MIDI THRU output signals are connected directly to MIDI IN connector

Resolution: Redesign MCU Interface PCB to allow FPGA to drive the MIDI THRU signals.