Problem Report PR-005

HW part: HW0001

HW rev: R002

Description: PCB hardware is not able to drive I2C signals.

Analysis to demonstrate the problem:

1. I2C2 signals SDA (MCU Pin 23) and SCL (MCU Pin 24) are not connected to connector J2.

Resolution: Jumper AN3 to SDA at J2-13 and AN2 to SCL at J2-11 so that the MCU Interface PCB can use them in this application. Add SDA to J2-13 and SCL to J2-11 on the MCU Interface PCB.